**SKMEI 1672 Operation Manual**



 **FEATURE**

* 24H time display (LED display)
* body temperature measurement (LED display)
![9EHDPRWVZMX9]SUE$ZWPLUV]()

Charging (the left symbol flash)

Normal Temperature

Time Display

Abnormal Temperature (the left symbol flash quickly)

1. **Time display**
* press S key to display the time, it automatically turns off to save electricity when there is no operation.
1. **Time setting**
* Under the mode of time display , keep pressing S key for 5 seconds to enter the setting of “Hour” then press S key again to modify the number of “hour”. Press S key and hold it for 5 seconds again to enter the setting of “ minute” then press S key to modify the number of “minute”.
1. **Test the temperature**
* Under the mode of time display, press S key to measure the temperature and the symbol ℃ flashes , symbol ℃ stop flashing after test finished.
* Attention: There are 2 abnormal results of measurements when the temperature is out of the range of 32℃~42.5℃: ①LO or HI means it too low temperature or too high temperature to be out of range of measurement.② Red light will flash when temperature exceeds 37.5℃。Within range of measurement.
* Measuring range is 34℃~42℃. Results of measurements will be affected individual difference, environment , clothing ,strenuous exercise and other factors . The result are for reference only and cannot be used as a basis for diagnosis .

**Remarks: Wear your watch for ten minutes before detecting your body temperature**;

1. **Charging**
* Take off wrist band and connect it with USB charging cable
* Led screen display : On charging : The left symbol flash
 Full charge : The left symbol stop flashing.